See: https://github.com/wemos/WEMOS_Motor_Shield_Arduino_Library/issues/1

Possible solution: Reprogram STM32 on the shield:
https://hackaday.io/project/18439-motor-shield-reprogramming

Can be done only with wemos:
https://github.com/thomasfredericks/wemos_motor_shield
