(footprint "Vishay_PowerPAK_MLP44-24L" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (property "Sheetfile" "bucker.kicad_sch")
  (property "Sheetname" "")
  (property "Sorting" "00")
  (attr smd)
  (fp_text reference "U1" (at -0.075 -3.025 -90 unlocked) (layer "F.SilkS") hide
      (effects (font (size 0.5 0.5) (thickness 0.1)))
    (tstamp b8f92d5d-a574-45d1-95e5-123c8e2be37f)
  )
  (fp_text value "SiC437" (at 0 3.3 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 530fdcc3-0cda-4bf1-a415-7060849acbce)
  )
  (fp_line (start -2.1 1.7) (end -2.1 2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7f3e784c-3900-460d-a176-6f8578d53cc2))
  (fp_line (start -2.1 2.1) (end -1.7 2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d09abfee-b553-4026-beba-33c23e64ce45))
  (fp_line (start -1.7 -2.1) (end -2.1 -2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 012b5395-6ef0-4444-b3fc-7a66a5c123df))
  (fp_line (start 1.7 2.1) (end 2.1 2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 21f8d6d2-2d6d-45fb-b2ee-e47a8557a845))
  (fp_line (start 2.1 -2.1) (end 1.7 -2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 436dcc85-9012-4afe-be03-3caca5f44f0f))
  (fp_line (start 2.1 -1.7) (end 2.1 -2.1)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a68be7fb-0a41-4b44-8e75-702cd5d81c41))
  (fp_line (start 2.1 2.1) (end 2.1 1.7)
    (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 41612b3b-8945-4803-bc0d-96a6d386c652))
  (fp_rect (start -2.5 -2.5) (end 2.5 2.5)
    (stroke (width 0.12) (type solid)) (fill none) (layer "F.CrtYd") (tstamp e27e0623-222e-4d44-9c0a-12d284b452b7))
  (fp_poly
    (pts
      (xy 2 2)
      (xy -2 2)
      (xy -2 -1)
      (xy -1 -2)
      (xy 2 -2)
    )

    (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 90ab20f2-9775-4e90-8038-2daaac466f6c))
  (pad "1" smd roundrect (at -1.9 -0.825) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp da148d37-5cb3-40b0-80fb-4c0a8eaa441d))
  (pad "1" smd roundrect (at -1.9 -0.375) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6befb469-10c6-41cc-8cd1-60b34ef29b7c))
  (pad "1" smd roundrect (at -1.175 -0.75) (size 1.15 1.05) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07142857143) (tstamp 40687068-d25e-40f4-bbe6-098d66d3c64a))
  (pad "3" smd roundrect (at -1.8 0.525) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0dcc64d4-b86a-4823-8841-b7029f784aec))
  (pad "3" smd roundrect (at -1.8 0.975) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8fa8a441-9fdc-4c08-a766-a5e5315bd477))
  (pad "3" smd roundrect (at -0.65 0.675) (size 2.175 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.08333333333) (tstamp 97154aac-866b-48d1-bba9-c3d2aa3ce136))
  (pad "3" smd roundrect (at 0.6625 0.3025) (size 0.85 0.455) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1648351648) (tstamp bcc4f109-c08b-453c-a391-e423aac0a7ce))
  (pad "5" smd roundrect (at -1.475 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp a027ff16-565b-4cfc-8cec-d2f7b6de6a6a))
  (pad "5" smd roundrect (at -1.025 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 71b08d81-a7c4-4786-9160-bc712eb7de1f))
  (pad "5" smd roundrect (at -0.575 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e370acf9-5e3f-4e49-a286-1c1a65eeae7e))
  (pad "5" smd roundrect (at -0.455 1.7125) (size 2 0.275) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1973672727) (tstamp 2b8b4645-834a-4dc2-bde0-b02c7448552d))
  (pad "5" smd roundrect (at 0.125 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0949cb00-0adc-4832-8114-f90609cb0d53))
  (pad "5" smd roundrect (at 0.575 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 609d4551-aa6e-4ff4-a251-bce1e03acb6d))
  (pad "10" smd roundrect (at 1.025 1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e6c8479d-8890-4300-bf68-59893e694cf7))
  (pad "11" smd roundrect (at 1.925 1.425) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 811b2763-bdaf-43a8-971b-50469a5f2d50))
  (pad "12" smd roundrect (at 1.925 0.975) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1cb8f2d4-bc27-450b-a254-57b99a3cf6f8))
  (pad "13" smd roundrect (at 1.925 0.525) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d2ee2251-acb0-455f-b397-406b99cfe879))
  (pad "14" smd roundrect (at 1.925 0.075) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d33bc44f-541e-49f2-adc0-cf8c173dfc28))
  (pad "15" smd roundrect (at 1.925 -0.375) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 1c1bc3ec-8425-46e0-ab3f-bcf622b8742a))
  (pad "16" smd roundrect (at 1.925 -0.825) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 9186dc61-91f8-4a0a-a3b7-e787badb3e53))
  (pad "17" smd roundrect (at 1.925 -1.275) (size 0.725 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4ea9946a-2561-4ee8-a793-f54d1f95618e))
  (pad "18" smd roundrect (at 1.475 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ff0ed24e-2c9f-42eb-8e87-cfe802c979a1))
  (pad "19" smd roundrect (at 1.025 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 2d681965-7d87-433c-b3e1-e5c62d7bf930))
  (pad "20" smd roundrect (at 0.575 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp daa90756-cb6e-4a55-8f6a-861f7a7c2da0))
  (pad "21" smd roundrect (at 0.125 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 0df4ae9c-8989-4613-9be1-f0477bf03fbb))
  (pad "22" smd roundrect (at -0.575 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 55a6cbde-721f-4ad6-94a2-9d38d84115de))
  (pad "23" smd roundrect (at -1.025 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 34366b28-3550-49e0-bd7c-cd5ee62a69f4))
  (pad "24" smd roundrect (at -1.475 -1.9375) (size 0.3 0.725) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d5c7894f-339d-4e97-9b65-313f444c19b9))
  (pad "25" smd roundrect (at 0.475 -0.75) (size 1.575 1.05) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07142857143) (tstamp 51a34a98-374c-46d1-9109-6da17cae5f6a))
  (pad "28" smd roundrect (at 0.985 0.99) (size 0.58 0.38) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1648342105) (tstamp f961fe77-6261-4f69-a4ec-56f0aa7b0b94))
)
